* It functions as a half-duplex serial port with a fixed baud rate123.
* The 8-bit serial data is received and transmitted through the RxD pin12.
* The controller outputs the shift clock through the TxD pin during reception and transmission12.
* The baud rate is fixed at 1/12 of the oscillator frequency123.